set use_usb_driver [expr [have_spec omap4] || [have_spec arndale] || [have_spec rpi]]
set use_nic_driver [expr [have_spec linux] || [expr !$use_usb_driver && ![have_spec imx53] && ![have_spec odroid_xu] && ![have_spec linux] && ![have_spec wand_quad]]]

requires_installation_of lynx

#
# Build
#

proc gpio_drv { } { if {[have_spec rpi] && [have_spec hw]}  { return hw_gpio_drv }
                    if {[have_spec rpi] && [have_spec foc]} { return foc_gpio_drv }
                    return gpio_drv }

set build_components {
	core init
	drivers/timer drivers/nic
	test/lxip/http_srv
}

lappend_if $use_usb_driver              build_components drivers/usb
lappend_if [have_spec gpio]             build_components drivers/gpio

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

build $build_components

create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="test-lxip_http_srv" caps="200">
		<resource name="RAM" quantum="28M"/>
		<config ld_verbose="yes">
			<vfs> <dir name="dev"> <log/> </dir> </vfs>
			<libc stdout="/dev/log" stderr="/dev/log" ip_addr="10.0.2.55" gateway="10.0.2.1" netmask="255.255.255.0"/>
		</config>
	</start>}

append_if [have_spec gpio] config "
	<start name=\"[gpio_drv]\">
		<resource name=\"RAM\" quantum=\"4M\"/>
		<provides><service name=\"Gpio\"/></provides>
		<config/>
	</start>"

append_if $use_usb_driver config {
	<start name="usb_drv">
		<resource name="RAM" quantum="12M"/>
		<provides>
			<service name="Nic"/>
		</provides>
		<config ehci="yes">
			<nic mac="02:00:00:00:01:01" />
		</config>
	</start>}

append_platform_drv_config

append_if $use_nic_driver config {
	<start name="nic_drv" caps="120">
		<binary name="} [nic_drv_binary] {"/>
		<resource name="RAM" quantum="20M"/>
		<provides><service name="Nic"/></provides>
	</start>}

append config {
</config>
}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core ld.lib.so init timer posix.lib.so
	libc.lib.so libm.lib.so lxip.lib.so test-lxip_http_srv
}

# platform-specific modules
lappend_if $use_usb_driver              boot_modules usb_drv
lappend_if $use_nic_driver              boot_modules [nic_drv_binary]
lappend_if [have_spec gpio]             boot_modules [gpio_drv]

append_platform_drv_boot_modules

build_boot_image $boot_modules

#
# Execute test case
#

# qemu config
append qemu_args "  -nographic "

append_if [have_spec x86]     qemu_args " -net nic,model=e1000 "
append_if [have_spec lan9118] qemu_args " -net nic,model=lan9118 "

append qemu_args " -net user -redir tcp:5555::80 "

 run_genode_until forever

set match_string "ipaddr=(\[0-9\]+\.\[0-9\]+\.\[0-9\]+\.\[0-9\]+).*\n"
run_genode_until $match_string 30

if {[have_include "power_on/qemu"]} {
	set uri "http://localhost:5555/"
} else {
	regexp $match_string $output all ip_addr

	set uri "http://$ip_addr:80/"
}

puts "http server is up, try to query website $uri"

set website [exec lynx -dump $uri]

puts "response:\n$website"

if {![regexp {Welcome to our HTTP demonstration server!} $website dummy]} {
	puts stderr "Query returned unexpected website"
	exit 2;
}

# vi: set ft=tcl :
