#
# Smartcard test
#
# NOTE: The vendor id and product id of the USB card reader to be used must be
#       configured for the application and for the USB driver.
#

if { [have_include "power_on/qemu"] || [have_spec linux] || [have_spec muen] } {
	puts "Run script does not support Qemu, Linux, and Muen"
	exit 0
}

assert_spec x86_64

#
# Please configure your reader's vendor and product IDs here
#
proc smartcard_vendor_id {}  { return "0x04e6" }
proc smartcard_product_id {} { return "0x5116" }

#
# Build
#

set build_components {
	core init timer
	drivers/usb
	test/smartcard
}

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

build $build_components

create_boot_directory

#
# Generate config
#

append config {
<config>
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>}

append_platform_drv_config

append config {
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>
	<start name="report_rom">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Report"/> <service name="ROM"/> </provides>
		<config verbose="no">
			<default-policy report="usb_drv -> devices"/>
		</config>
	</start>

	<start name="usb_drv" caps="200">
		<resource name="RAM" quantum="16M"/>
		<provides><service name="Usb"/></provides>
		<config uhci="yes" ehci="yes" xhci="yes" bios_handoff="yes">
			<raw>
				<report devices="yes"/>
				<policy label="test-smartcard -> usb_device"
				        vendor_id="} [smartcard_vendor_id] {" product_id="} [smartcard_product_id] {"/>
			</raw>
		</config>
		<route>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

	<start name="test-smartcard" caps="150">
		<resource name="RAM" quantum="4M"/>
		<config>
			<vfs>
				<dir name="dev"> <log/> <inline name="rtc">2018-01-01 00:01</inline> </dir>
				<dir name="ifd-ccid.bundle">
					<dir name="Contents">
						<rom name="Info.plist"/>
					</dir>
				</dir>
			</vfs>
			<libc stdout="/dev/log" stderr="/dev/log" rtc="/dev/rtc"/>
			<env key="LIBUSB_DEBUG" value="1"/> <!-- log libusb errors -->
		</config>
	</start>
</config>}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core init timer usb_drv test-smartcard
	ld.lib.so pcsc-lite.lib.so ccid.lib.so libusb.lib.so
	libc.lib.so vfs.lib.so libm.lib.so libc_pipe.lib.so posix.lib.so
	Info.plist
}

append_platform_drv_boot_modules

build_boot_image $boot_modules

run_genode_until { Response: 62 0A 82 01 38 83 02 3F 00 8A 01 05 90 00} 30

exec rm bin/Info.plist
