assert_spec acpi

if {
	![have_spec hw] &&
	![have_spec nova] &&
	![have_spec sel4]
} {
	puts "Platform is unsupported."
	exit 0
}

set build_components {
	core init timer
	drivers/input
	server/acpi_input
	server/dynamic_rom
	server/input_filter
	server/report_rom
	app/acpica
	test/input
}

set use_acpica_as_acpi_drv 0

source ${genode_dir}/repos/base/run/platform_drv.inc

if {!$use_acpica_as_acpi_drv} {

	# override default platform driver policy
	proc platform_drv_policy {} {
		return {
				<policy label_prefix="ps2_drv"> <device name="PS2"/> </policy>
				<policy label_prefix="acpica"> <pci class="ALL"/> </policy>}
	}

	# add routing information
	proc platform_drv_add_routing {} {
		return {
				<service name="ROM" label="acpi_ready"> <child name="acpi_state"/> </service>}
	}

	# override default config to react on 'acpi_ready' ROM change
	proc platform_drv_config_config {} {
		return {
			<config acpi_ready="yes">}
	}
}

append_platform_drv_build_components

build $build_components

create_boot_directory

set config {
	<config>
		<parent-provides>
			<service name="IRQ"/>
			<service name="ROM"/>
			<service name="LOG"/>
			<service name="RM"/>
			<service name="PD"/>
			<service name="CPU"/>
			<service name="IO_MEM" />
			<service name="IO_PORT" />
		</parent-provides>
		<default-route>
			<any-service> <parent/> <any-child/> </any-service>
		</default-route>
		<default caps="100"/>
		<start name="timer">
			<resource name="RAM" quantum="2M"/>
			<provides><service name="Timer"/></provides>
		</start>}

append_if [expr !$use_acpica_as_acpi_drv] config {
		<start name="acpica" caps="150">
			<resource name="RAM" quantum="5M"/>
			<config ld_verbose="yes" reset="no" poweroff="no" report="yes" acpi_ready="yes">
			</config>
			<route>
				<service name="ROM" label="system"> <child name="dynamic_rom"/> </service>
				<service name="Report">  <child name="acpi_state"/> </service>
				<any-service> <parent/> <any-child/> </any-service>
			</route>
		</start>}

append config {
		<start name="acpi_state">
			<binary name="report_rom"/>
			<resource name="RAM" quantum="2M"/>
			<provides>
				<service name="ROM" />
				<service name="Report" />
			</provides>
			<config verbose="yes">
				<policy label="platform_drv -> acpi_ready" report="acpica -> acpi_ready"/>
				<policy label="acpi_input -> acpi_ac" report="acpica -> acpi_ac"/>
				<policy label="acpi_input -> acpi_battery" report="acpica -> acpi_battery"/>
				<policy label="acpi_input -> acpi_ec" report="acpica -> acpi_ec"/>
				<policy label="acpi_input -> acpi_fixed" report="acpica -> acpi_fixed"/>
				<policy label="acpi_input -> acpi_lid" report="acpica -> acpi_lid"/>
			</config>
			<route>
				<any-service> <parent/> </any-service>
			</route>
		</start>}

append config {
		<start name="dynamic_rom">
			<resource name="RAM" quantum="4M"/>
			<provides><service name="ROM"/></provides>
			<config verbose="yes">
				<rom name="system">
					<inline description="set system state to 'normal'">
						<system state="normal"/>
					</inline>
					<sleep milliseconds="5000" />
					<inline description="set system state to 'reset'">
						<system state="reset"/>
					</inline>
<!--
					<inline description="set system state to 'poweroff'">
						<system state="poweroff"/>
					</inline>
-->
					<sleep milliseconds="500" />
				</rom>
			</config>
		</start>}

append config {
		<start name="input_filter">
			<resource name="RAM" quantum="1M" />
			<provides> <service name="Input" /> </provides>
			<config>
				<input label="ps2" />
				<input label="acpi" />
				<output>
					<merge>
						<input name="ps2"/>
						<input name="acpi"/>
					</merge>
				</output>
			</config>
			<route>
				<service name="Input" label="ps2"> <child name="ps2_drv" /> </service>
				<service name="Input" label="acpi"> <child name="acpi_input" /> </service>
				<any-service> <parent/> </any-service>
			</route>
		</start>}

append config {
		<start name="ps2_drv">
			<resource name="RAM" quantum="2M"/>
			<provides><service name="Input"/></provides>
			<config verbose_keyboard="no" verbose_mouse="no" verbose_scancodes="no"/>
			<route>
				<service name="Platform"> <child name="platform_drv"/> </service>
				<service name="Timer"> <child name="timer"/> </service>
				<any-service> <parent/> </any-service>
			</route>
		</start>

		<start name="test-input">
			<resource name="RAM" quantum="1M"/>
			<route>
				<service name="Input"> <child name="input_filter"/> </service>
				<service name="Timer"> <child name="timer"/> </service>
				<any-service> <parent/> </any-service>
			</route>
		</start>}

append config {
		<start name="acpi_input">
			<resource name="RAM" quantum="1M"/>
			<provides><service name="Input"/></provides>
			<config>
				<!-- example mapping - adapt to your target notebook !!! -->
				<!-- as="PRESS_RELEASE" is default if nothing specified -->
				<map acpi="ec"      value="25"      to_key="KEY_VENDOR"/>
				<map acpi="ec"      value="20"      to_key="KEY_BRIGHTNESSUP"/>
				<map acpi="ec"      value="21"      to_key="KEY_BRIGHTNESSDOWN"/>
				<map acpi="fixed"   value="0"       to_key="KEY_POWER"  as="PRESS_RELEASE"/>
				<map acpi="lid"     value="CLOSED"  to_key="KEY_SLEEP"  as="PRESS"/>
				<map acpi="lid"     value="OPEN"    to_key="KEY_SLEEP"  as="RELEASE"/>
				<map acpi="ac"      value="ONLINE"  to_key="KEY_WAKEUP"/>
				<map acpi="ac"      value="OFFLINE" to_key="KEY_SLEEP"/>
				<map acpi="battery" value="0"       to_key="KEY_BATTERY"/>
			</config>
			<route>
				<service name="ROM" label="acpi_ac"> <child name="acpi_state"/> </service>
				<service name="ROM" label="acpi_battery"> <child name="acpi_state"/> </service>
				<service name="ROM" label="acpi_ec"> <child name="acpi_state"/> </service>
				<service name="ROM" label="acpi_fixed"> <child name="acpi_state"/> </service>
				<service name="ROM" label="acpi_lid"> <child name="acpi_state"/> </service>
				<any-service> <parent/> </any-service>
			</route>
		</start>}

append_platform_drv_config

append config {
</config>
}

install_config $config

set boot_modules {
	core init
	ld.lib.so
	timer
	ps2_drv
	input_filter
	report_rom
	dynamic_rom
	acpica
	acpi_input
	test-input
}

append_platform_drv_boot_modules

build_boot_image $boot_modules

append qemu_args "-nographic "

run_genode_until {\[init -\> acpi.*SCI IRQ:.*\n} 30
