#
# \brief  Test for using the lwIP TCP/IP stack over USB
# \author Sebastian Sumpf
# \date   2012-07-06
#
# This test case executes a small HTTP server, it has been used on PandaBoard
# hardware only, though it should execute but not do anything on other hardware
#

#
# Build
#

build {
	core init
	drivers/pci drivers/timer drivers/usb
	test/lwip/http_srv
}

lappend_if [have_spec acpi]             build_components drivers/acpi
lappend_if [have_spec pci]              build_components drivers/pci/device_pd
lappend_if [have_spec platform_arndale] build_components drivers/platform
lappend_if [have_spec gpio]             build_components drivers/gpio


create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="RAM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="CAP"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
		<service name="SIGNAL"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="usb_drv">
		<resource name="RAM" quantum="12M"/>
		<provides>
			<service name="Nic"/>
		</provides>
		<config ehci="yes">
			<nic mac="2e:60:90:0c:4e:01" />
		</config>
	</start>
	<start name="test-lwip_httpsrv">
		<resource name="RAM" quantum="2M"/>
	</start>}

append_if [have_spec acpi] config {
	<start name="acpi">
		<resource name="RAM" quantum="5M"/>
		<binary name="acpi_drv"/>
		<provides>
			<service name="PCI"/>
			<service name="IRQ" />
		</provides>
		<route>
			<service name="PCI"> <any-child /> </service>
			<any-service> <parent/> <any-child /> </any-service>
		</route>
	</start>}

append_if [have_spec platform_arndale] config {
		<start name="platform_drv">
			<resource name="RAM" quantum="1M"/>
			<provides><service name="Regulator"/></provides>
		</start>}

append_if [have_spec gpio] config {
	<start name="gpio_drv">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="Gpio"/></provides>
		<config/>
	</start>}

append_if [expr ![have_spec acpi] && [have_spec pci]] config {
	<start name="pci_drv">
		<resource name="RAM" quantum="3M"/>
		<provides> <service name="PCI"/> </provides>
	</start> }

append config {
</config>
}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core init timer
	usb_drv
	ld.lib.so libc.lib.so libc_log.lib.so lwip.lib.so test-lwip_httpsrv
}

lappend_if [have_spec acpi]             boot_modules acpi_drv
lappend_if [have_spec pci]              boot_modules pci_drv
lappend_if [have_spec nova]             boot_modules pci_device_pd
lappend_if [have_spec platform_arndale] boot_modules platform_drv
lappend_if [have_spec gpio]             boot_modules gpio_drv

build_boot_image $boot_modules

run_genode_until forever
# vi: set ft=tcl :
