#
# Build
#

# generic components
set build_components {
	core init
	drivers/timer
	drivers/sd_card
	test/block
}

build $build_components
create_boot_directory


#
# Config
#

set config  {
	<config>
		<parent-provides>
			<service name="ROM"/>
			<service name="RAM"/>
			<service name="IRQ"/>
			<service name="IO_MEM"/>
			<service name="CAP"/>
			<service name="PD"/>
			<service name="RM"/>
			<service name="CPU"/>
			<service name="LOG"/>
			<service name="SIGNAL"/>
		</parent-provides>
		<default-route>
			<any-service> <parent/> <any-child/> </any-service>
		</default-route>

		<start name="timer">
			<resource name="RAM" quantum="1M"/>
			<provides><service name="Timer"/></provides>
		</start>
		<start name="sd_card_drv">
			<resource name="RAM" quantum="1M"/>
			<provides><service name="Block"/></provides>
		</start>
		<start name="test-block">
			<resource name="RAM" quantum="1M" />
		</start>
	</config>
}

install_config $config


#
# Boot modules
#

# generic modules
set boot_modules {
	core init
	timer
	sd_card_drv
	test-block
}

set disk_image "bin/sd_card.img"

build_boot_image $boot_modules
append qemu_args "-drive file=$disk_image,if=sd,cache=writeback -nographic "

if { [file exists $disk_image] == 0 } then {
	# create empty block device file
	catch { exec dd if=/dev/zero of=$disk_image bs=1M count=512 }
}

run_genode_until forever

# vi: set ft=tcl :
